





Mounting the Solar Panels to the Roof


GSE Integration offers a fast, elegant and universal mounting system for panels



Pantile installations use the 176mm fixings




Permits both portrait and landscape mounting




Maximum spacing is 200cm.

Maximum cantilever is 60cm

Pantiles are modified with a single hole

Tube glued in place at correct length

Attaching rail to rail support



Attachment of PV panels to rails

