**Outdoor CCTV product proposed for 61 Avenue Road.**

* Product can be supplied in black, white or grey finish (to best match mounting walls).
* All cameras are static type (no Pan & Tilt)
* All cameras have built in supplementary lighting, no additional external lighting required for night time operation is required.
* All devices are copper cabled (no wireless). No cables will be visible as devices mount over cable entry/exit point.
* Devices fit directly to the house/perimeter walls (no additional bracketry required).
* Projection from walls will not exceed 150mm.
* Distance above ground level for all front elevation devices will not exceed 3m.
* Distance above ground level for rear elevation devices will not exceed 7m.
* Distance above ground level for perimeter devices will not exceed 2m.

Number of devices per elevation, as per attached drawings:

**Front of House**

6 x cameras

2 x speakers

4 x PIR

**Rear of House**

7 x cameras

2 x speakers

4 x PIR

**Boundary Perimeter**

6 x cameras

3 x PIR

4 x Thermal cameras (optional)

