**Erection of Summerhouse.**

Erection of timber summerhouse in northeast corner of site as shown on plan. Dimensions 4mx 3m with pent roof maximum height 2.5m vertical larch cladding left to weather naturally with insulated profile sheet steel roof in slate grey. Windows to north, east and west elevations with door and sidescreen in North elevation. See plan B for location and Plan SH1 for plan and elevations.