PROPOSED REPLACEMENT OF BOX SASH WINDOWS FOR 41 LONDON ROAD, SEVENOAKS

Reference no. PP-0923588 – K.GOLDING

Specifications:

1. Kiln dried Sapele/Utile on all timber components
2. Make up of manufacture, like for like in accordance with sound joinery practice Ref. C.F.C Webber Carpentry & Joinery Published 1898 Fourth edition. Publisher Methuem & Co.
3. Section sizes (all sizes mm)
* Pulley styles 22X86
* Pulley Head 22X86
* Inner casing 19X78
* Outer casings 19 x94
* Parting Bead 7X22
* Stop/staff Beads 16X22
* Parting laths/slips 6X50
* Back lings 6X108
* No brackets
* Sash styles 39X44
* Top rails 39X44
* Meeting rail 39X22
* Bottom rail 39X64
* Glazing bar 26X39
* Bottom sill 64X125
1. Draught seals
* 5mm brush pile fitted to

Top sash head rail

Top sash parting rail

Parting Beads

Stop/staff Beads

1. Ironmongery
* Solid brass pulleys with bearings
* Finch locks solid brass
1. Sash cord 8mm polyester
2. Glazing
* Glass 4mm toughened float/3mm rolled as directed by Conservation Officer
* Non-toxic putty
1. Painting
* Paint Zinsser Allcoat 1 primer, 1 undercoat, 2 topcoats
* Paint specifications – see attachment
* Paint carries a 15 year guarantee
* Environment and H&S compliance – see attached COSH data
1. Fixings
* Screws – stainless steel
* Pins – galvanised
1. Adhesive
* Waterproof Wurth D4
1. Waste Removal
* Removal to a registered waste site in Sevenoaks, Kent.