**Details of Work Required/Recommended**

Tree number - G1 shown on drawings as T15

Tree type - Cypress x2

Approx Height - 7m

Location - see aerial photo and plan

Service - Fell and grind

Work required - Fell and grind out stump to a depth of approx. 200mm below the stumps

current ground level and leave all stump's arising to allow for ground settlement

Tree Number - T1 shown on drawings as T14

Tree Type - Ash

Approx Height - 12m

Location - see aerial photo and plan

Service - Cut Back

Work required - crown lift all round to approximately 4m. Cut back remainder back to

boundary by removing approximately 2-3m from applicants side only.

All resulting brushwood and logs will be transported to the contractors recycling depot awaiting transfer to be used as bio-fuel **(unless otherwise stated in work description above).**