A close-up of a bag

Description automatically generated

**Base Coat**

Applied To Waterproofing Membrane – 12-15mm. In Thickness