
A roof with a window

Description automatically generatedDorner Pitched ~Roofs

The dormer roofs are low pitched and not suitable for Plain Clay tiles – the proposal is to repalce these with Del Carmen Spanish slate 10”x20” – With 50mm core roll ridge clad in Code 6 Sand Cast Lead



Vent Pipes to be removed and replaced with discrete Palin tile Vents

