**Planning Application DC/21/02051**

1. **Front Fence Panels: Framed Willow Panels (Straight Topped)**

Manufacturers specification:

Width: 1.8m

Height: 1.5m

Depth: 4cm

Supplier: Nelson Potter Limited

Supplier Description:

Heavy duty & Robust

Fully Framed treated timber

Half lapped frame

Traditional with the Rustic effect

Hand Weaved Willow

Imported from a regularly harvested plantation

Please note: as this is a natural product and you may notice variations in colour.

See Figure 1

1. **Back Fence Panels: Closeboarded Timber panels (Imported W/Board Panels)**

Manufacturers specification:

Width: 1.828m

Height: 1.525m

Depth: 4cm

Supplier: Nelson Potter Limited

Supplier Description:

Imported W/Board panels fully framed & half lapped using 60mm x 27mm timbers

Fully framed & half lapped using 60mm x 27mm timbers

Heavy duty W/Board using 2ex 125mm x 22mm

Weather capping top rail nailed with Galvanised ring shank nails

Pressure treated in green

See Figure 2

1. **Wood Gavel Boards – to be positioned under all fencing**

Manufacturers specification:

Height: 150mm

Depth: 22mm

Supplier: Nelson Potter Limited

Supplier Description: Pressure treated in ACQ Green – conforms toUC3(BSEN3351)

1. **Softwood Timber fence posts (Brown) – to be used for all fence and gate panels**

Manufacturers specification:

100mm x 100mm square posts

Supplier: Nelson Potter Limited

Supplier description:

All 100 % Pine (Redwood)

Dried to an average of 28% moisture content prior to treatment

Pressure treated in ACQ Green or Brown to UC4)

1. **Front Fence Gate: Framed Willow Garden Gate (bespoke)**

Manufacturers specification:

Width: 0.915m

Height: 1.5m

Depth:10cm

Description:

Frame, Ledge & Braced Pedestrian Gate

Heavy duty & Robust

Utilising Willow fence panel or willow screening

Traditional with the Rustic effect

Hand Weaved Willow

See Figure 3



Figure 1: Framed Willow Panel – Front Fence



Figure 2: Closedboarded panel (back fence)



Figure 3: Framed Willow Gate for Front Fence access