

**Mr & Mrs Macleod**

**Re: Sash lights**

**Position Width Height Notes**

FF1 L/H Bed 1010mm 1742mm Bottom light opens, top light fixed

Bottom light clear tough, top clear annealed

6 over 6

FF2 R/H Bed 1010mm 1732mm Bottom light opens, top light fixed

Bottom light clear tough, top clear annealed

6 over 6

GF1 Pantry 1036mm 1755mm Bottom light opens, top light fixed

Bottom light clear tough, top clear annealed

Unscrew metal bars on inside (slotted)

6 over 6

GF2 Kitchen 1327mm 1740mm Bottom light opens, top light fixed

Bottom light clear tough, top clear annealed

No pulley slots on bottom light

8 over 8

GF2 Study 1327mm 1740mm Bottom light opens, top light fixed

Bottom light clear tough, top clear annealed

Resin repairs

8 over 8

All sizes are tight boxes, allowance needs to be made. 6mm narrower in the width and 0mm in the height

**Notes:**

No repairs to existing boxes have been allowed except on the study window. Any work to these will be charged at time and materials

**A.R MANLEY & SON LTD**

**SOMERWOOD . RODINGTON . Nr.SHREWSBURY . SY4 4RF**

**TELEPHONE: (01952) 770278**

WEB SITE: [www.armanley.co.uk](http://www.armanley.co.uk) . EMAIL: [sales@armanley.co.uk](mailto:sales@armanley.co.uk)

REGD NO 596052 . VAT REGD NO. 159 3473 39