Proposed Lighting Specification

2 lights proposed per column

Specification:

Lights are 100w

Colour temp 4000k

Size 310 x 260 x 70 mm

Cri 80

Output 0.22a

Frequently 50-60Hz

Max output current 1.1a

Beam angle 120 degrees

Ip65

Energy Efficiency A++ (2021)

Energy Efficiency D (2023)

Lumens 13000lm