**GOOSE ACRE**

Land Rear Of Gooseacre Buckwood Road Markyate AL3 8JD


Application - 4/01283/19/FUL

Condition 3 – External Wall Materials

**EXTERNAL WALLS**

To be constructed from waste brick sourced from H.G. Matthews brickworks. Exact colour and type will depend on the particular waste products. A Sample panel has been constructed at the offices of Kirkland Fraser Moor, Berkhamsted. Alternatively, a new Para 80 dwelling at Wiggington has recently been completed using the same technique and materials. This can demonstrate the proposals over a larger area.

*Waste Brick Walls*



Goose Acre sample at KFM Studio, Berkhamsted.

Example from Park Farm (Para 80) House. Wiggington.



Other cladding will include standard Timber Clad Walls (Black Stained). . Samples available at KFM Studio Berkhamsted.

*Glazing*

Glazing will be high performance anodized aluminium glazing. To be determined following technical design.

*Details*

Parapets and wall details will be reconstituted Portland Stone. Samples available at KFM Studio Berkhamsted.