TREE WORK Edgware Abbey

T1 Horsechestnut St Johns House

Goals:

• Remove disease dead wood

• Reduce size of crown height and spread

Specifications:

• Reduce live branches as needed, 0.2-0.5 metres length reduction, entire canopy

• Remove dead branches as needed, entire canopy

T2 Ash St Giberts Area

Goals:

• Reduce height and spread of tree by pollarding back to previous pruned points

Specifications:

• Remove live branches as needed, entire canopy

T3 Ash Boundary fence line

Goals:

• Reduce height and spread of tree by pollarding back to previous pruned points

Specifications:

• Remove all live branches, entire canopy

T4 Hawthorn St Gilberts shed area

Goals:

• Remove disease dead wood

• Reduce size of crown height and spread

• Reduce density

Specifications:

• Remove all dead branches, entire canopy

• Reduce live branches as needed, 1-2 metres length reduction, entire canopy

• Reduce and/or remove 10 percent of live, rubbing branches, entire canopy

T5 Ginkgo Cemetery Area inner court yard

Goals:

• Provide of clearance

Specifications:

• Remove live branches as needed, growing toward building

T6 Cherry Cemetery

T7 Cherry Cemetery

T8 Crabapple Cemetery

Reduce size of crown height and spread

Specifications:

• Reduce all live, over-extended branches, 1-2 metres length reduction, entire canopy

TG9 Maple X2 Silver birch X4 Hawthorne X1 front grass area mound

Goals:

• Remove disease dead wood

• Reduce density

T10 Beech Front grass area

T11 Beech Front grass area

Goals:

• Improve appearance

Specifications:

• Reduce and/or remove live, over-extended branches as needed, entire canopy formative prune

• Improve appearance

Specifications:

• Remove dead branches as needed, entire canopy

• Reduce and/or remove 15 percent of live, rubbing branches, entire canopy

T12 Horsechestnut front of property

Goals:

• basal and epicormic growth

Specifications:

• Remove live branches as needed, entire canopy

T13 Oak front of property

Goals:

• Remove disease dead wood

• Reduce crown height

• Reduce spread of crown

• Reduce density

Specifications:

• Remove dead branches as needed, entire canopy

• Reduce live, diseased branches as needed, 2-2.5 metres length reduction, center of canopy

• Reduce live, over-extended branches as needed, 2.5-3.5 metres length reduction, growing toward building and out door area

• Reduce and/or remove 10 percent of live, diseased, rubbing branches, entire canopy

T14 Magnolia front of property (peggy and douglas)

Goals:

• Reduce size of crown height and spread

Reduce live, interfering, over-extended branches as needed, 0.5-1 metres length reduction, entire canopy

• Reduce and/or remove 10 percent of live, rubbing, interfering branches, entire canopy

T15 Laburnum Right Side garden area

Goals:

• Improve appearance

• Reduce density

Specifications:

• Reduce live, over-extended branches as needed, 0.5-1 metres length reduction, entire canopy

• Reduce and/or remove 10 percent of live, rubbing, interfering, over-extended branches, entire canopy

**T16 Silver birch** by steps

**Goals:**

Reduce density

**Specifications:**

• Reduce and/or remove 10 percent of live, rubbing, interfering, over-extended branches, entire canopy

**17 Hawthorn** Rear Car Park area

**Goals:**

• Reduce size of crown height and spread

• Reduce density

**Specifications:**

• Reduce live, interfering, over-extended branches as needed, 1-2 metres length reduction, entire canopy

**Species Location**

**T18 Cherry** Rear Car Park area

**Goals:**

• Reduce size of crown height and spread

• Reduce density

**Specifications:**

• Reduce live, rubbing, interfering, over-extended branches as needed, 1.5-2.5 metres length reduction, entire canopy

**Species Location**

**TG19 Lime X5 Beech X3 Rowan X1** left side drive way in

**Goals:**

• Formatively prune

• Remove disease dead wood

• Provide of clearance

**Specifications:**

• Reduce and/or remove live, rubbing, interfering, over-extended branches as needed, 0.5-1 metres length reduction, entire canopy

• Remove all dead branches, entire canopy

• Reduce and/or remove live, over-extended branches as needed, lower branches lift to a height of 3m over drive way

**TG20 Cherry X2 Maple X1 Ash X1** left side top of drive in

**Goals:**

• Reduce spread of crown

• Provide of clearance

**Specifications:**

• Reduce all live, over-extended branches, 2-2.5 metres length reduction, growing toward and over drive way